			ERAIO: Ericsson AllinOne
			\----------------------/

                              Version 0.95
						by Darktelecom
					(darktelecom@portugalmail.pt)


-> 1. What is Eraio and what is supposed to do ?
-> 2. Current supported functions
-> 3. Receive LATEST Version FREE allways (see conditions bellow)
-> 4. Whats Next ? 
-> 5. *** How to use Eraio *** (NEW)
-> 6. Known problems

1. Eraio is the short name for Ericsson AllinOne.
   The targed of this project is to deliver a full range of services
   for all Ericsson mobile phones all in one software.
   The number and kind of services offered by this software can grow
   as customers might need. To receive latest version see point 3.
   Eraio was made and the copyright belongs to Darktelecom.
   Please check my website for more news at www.darktelecom.com 
					    www.come.to/darktelecom	

2. Eraio supports a large number of features. Latest released version
   until the current date offers the services marked with X.
   In addition you should also check Eraio page in www.darktelecom.com
   which is constantly updated and offers you more.
   Im working in all other features and i wish to support them in a
   near future. If you know how to implement any of the missing
   functions, please email me (darktelecom@portugalmail.pt). 
    

                 3xx    6xx/7xx      8xx  A1018  T10/T18 T28 R320  R250 R310 2618s
Enter Test        X        X          X     X       X     X    X
Exit Test         X        X          X     X       X     X    
Flash                      X          X     X       X     X    X
Net On            X        X          X     X       X     X    X
Net Off           X        X          X     X       X     X    X
Net Unlock        X        X
Net Lock                                                        
Phone Code Reset  X        X                X       X     X    X
Eeprom Upload              X                X
Eeprom Download            X                X       X     X    X
Decoded CODES        nck,nsck,phone       phone   phone phone 
Welcome Message   X        X          X     X       X     X    X
Batch Job	                            X       X     X    X
*Change IMEI                                X       X     X    X

>>>> Changing the IMEI doesnt correct the checksum, so dont use it yet !!

3. Im giving the LATEST version to all the guys who help me..
   How can you help me ? Well, i need phones for tests.
   This include the following models: 2618s,R250,R310,T10,T28.
   I want to fully support them, so i need the phones.
   Send me one of the phones mentioned and you will receive
   Eraio for free.

4. Whats next ? Well that is up to you!
   Support me and i will support you !
   I will work on more features and full support of all phones.
   Send comments and critics to darktelecom@portugalmail.pt.
   I will not answer to stupid question like: "Can you give it to me
   for free? I dont have phones for you and i cannot help you of
   another way! I just want the software!"
   Guys, i have lost a lot of time developing this and other software
   and im not going to give it without having nothing in return.
   Thanks for understanding.

5. *** How to use Eraio ***

  .If you want to
    - change the welcome message
    - download/upload eeprom
    - turn on/off netmonitor
    - un/lock from SP
    - reset phone code
    - change IMEI
    - do a batch job

    You must first enter test mode by pressing "ENTER TEST" and then you
    should click the button of the function you want to do.
    When you are finished, press "EXIT TEST" to leave test mode.
    Then you can turn your phone on if you want to.

  .If you want to
    - flash phone and update the software

    You dont have to click "ENTER TEST". Just press "FLASH PHONE" and follow
    instructions. Eraio currently supports *.SHX (Motorola hex format)  and
    *.SBN (Zulea ATRServ from http://www.zulea.com) files. Please note that
    some .SHX files are not correctly formated so Eraio can give some error
    while loading the flash file. This happens because some flash converters
    forget to insert a line in the end of a line containing "Sxxxxxxx" and
    then the .SHX stays with a line like "SxxxxxSxxxxxx" which will cause an
    error in the loading process. You can fix this by opening the .SHX file
    and when you find two lines in just one BIG line you should give an Enter
    before the second "Sxxxxxx". Maybe ill implement a way to fix the bad
    formatted .SHX files in the future.

   .If you want do
     - do a batch job

    Well this is implement only on A1018,T1x,T28 for now. After pressing the
    button "ENTER TEST", you can do a batch job. You can read an address of
    the EEPROM for example. To do that select "Read" in the listbox, write
    the address in the address box and the number of bytes you want to read
    (starting at the address you specified) writting that number in the count
    box. You can also write to an address of the EEPROM the same way. This
    time the number in the count box, if more than one, acts like a fill, so
    you can fill a range of addresses (starting at the address you specified
    and ending "count" bytes after) with the number of the "value box".
    You have another option that is "SWRITE" (special write).
    This time, the bytes being written to the EEPROM address specified have
    to be written in the "Dump/Special Window". The bytes have to be written
    in capitalised HEX format. Lets supose that you want to write to the
    address 0x0100 the following bytes FF 00 11 20. In this case you should
    enter in the "Dump/Special Window"   FF001120  (hex format, no spaces).
    
   .If the phone doesnt enter test mode, or other strange thing

    Take the phone from the cable, take the battery off, put back the
    battery and reconnect to the cable. Retry now. If the problem is still
    there please check the power of the battery. You should use a battery
    full charged or you can get strange errors.


6. Known problems

   Well, sometimes when adding new features, coders also add new bugs.
   From my experience with Eraio ive faced with some problems, which
   might also appear to you. Some are my fault and some are not.

   Some might be:
     - related to enter Test Mode (specially in 8x8 phones)
     - related to flashing with SHX files 
        (which can be fixed! read point 5)
     - phone doesnt turn on. Well, this wont almost for sure happen to
       you, but some guys screw up phone's eeprom. Most of the times,
       its impossible to update the eeprom by cable.
       Be carefull when changing eeprom contents by cable!
       The only way to fix this is by programming the eeprom manually.
     - possibly one or two more :)
 

                        Darktelecom, October/2000
 		       http://www.darktelecom.com
